

Fishhawk Falls

Flash BIOS SOP


1. Disable ME (There are two ways to disable ME):
2. HW disable ME:
3. Power off.
4. Look for the "ME UPDATE" jumper on the Motherboard.




1. Set "ME UPDATE" jumper to disable ME.



1. Power on.
2. Setup Menu disable ME:
3. Boot to Setup Menu "Chipset -> Workstation ME Configuration -> Firmware Update Configuration" page.



1. Set "Me FW Image Re-Flash" to Enabled and save and restart **(Only disable ME once)**.
2. Boot to Setup Menu "Chipset -> Workstation ME Configuration" page to check ME Status.



1. Save & Restart.
2. Boot to shell.
3. Go to BIOS package folder.
4. Run f.nsh to do flash.